##-----------------------------------------------------------------------------
## base.txt - fli4l configuration parameters                       3.0.1
##
## You can edit/change this file with any text editor.
##
##        P L E A S E   R E A D   T H E   D O C U M E N T A T I O N ,
##                      S E E   R E A D M E . T X T
##
##        B I T T E  U N B E D I N G T   D I E   D O K U M E N T A T I O N
##              L E S E N ,  S I E H E   R E A D M E . T X T
##
## Creation:     26.06.2001  fm
## Last Update:  $Id: base.txt 11071 2006-02-23 13:46:01Z hh $
##
## Copyright (c) 2001-2005 Frank Meyer <frank@fli4l.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##-----------------------------------------------------------------------------

#------------------------------------------------------------------------------
# General settings:
#------------------------------------------------------------------------------
HOSTNAME='fli4l'               # name of fli4l router
PASSWORD='admin'               # password for root login (console, sshd, imond)
BOOT_TYPE='hd'                 # boot device: fd, fdx2, dualfd, hd, cd, ls120,
                               # integrated, attached, netboot, pxeboot
                               # (cd, cdemul, hd and ls120 need an
                               # installed opt hd)
MOUNT_BOOT='rw'                # mount boot device (floppy): ro, rw, no
TIME_INFO='MEZ-1MESZ,M3.5.0,M10.5.0'
                               # description of local time zone,
                               # don't touch without reading documentation
KERNEL_VERSION='2.4.32'        # kernel version
KERNEL_BOOT_OPTION=''          # append option to kernel command line
COMP_TYPE_KERNEL='gzip'        # compression-type for kernel: gzip, bzip2
COMP_TYPE_ROOTFS='gzip'        # compression-type for rootfs: gzip, bzip2
IP_CONNTRACK_MAX=''            # override maximum limit of connection
                               # tracking entries
POWEROFF_ON_HALT='no'          # power off after shutting down the machine
REAL_MODE_POWEROFF='no'        # switch to real mode before invoking
                               # apm power off

#------------------------------------------------------------------------------
# Localisation
#------------------------------------------------------------------------------
LOCALE='de'                    # defines the default language for several
                               # components, such as menu and httpd

#------------------------------------------------------------------------------
# Mount extra floppy drive to /floppy:
#------------------------------------------------------------------------------
OPT_MOUNTFLOPPY='no'           # mount extra floppy drive: first, second, no

#------------------------------------------------------------------------------
# Console settings (serial console, blank time):
#------------------------------------------------------------------------------
CONSOLE_BLANK_TIME=''          # time in minutes (1-60) to blank
                               # console; '0' = never, '' = system default
SER_CONSOLE='no'               # use serial interface instead of or as
                               # additional output device and main input device
    SER_CONSOLE_IF='0'         # serial interface to use, 0 for ttyS0 (COM1)
    SER_CONSOLE_RATE='9600'    # baudrate for serial console
    SER_BEEP='no'              # enable beep after boot and shutdown

#------------------------------------------------------------------------------
# Debug Settings:
#------------------------------------------------------------------------------
DEBUG_STARTUP='no'             # write an execution trace of the boot
DEBUG_LOG=''                   # sequence to file DEBUG_LOG or console if
                               # DEBUG_LOG is empty

#------------------------------------------------------------------------------
# Show service menu after login:
#------------------------------------------------------------------------------
OPT_MENU='yes'                 # service menu for users
    MENU_LANGUAGE=''           # language for the service menu; defaults to
                               # 'LOCALE' if left empty
#------------------------------------------------------------------------------
# Keyboard layout
#------------------------------------------------------------------------------
KEYBOARD_LOCALE='auto'         # auto: use most common keyboard layout for
                               # the language specified in 'LOCALE'
OPT_MAKEKBL='no'               # set to 'yes' to make a new local keyboard
                               # layout map on the fli4l-router

#------------------------------------------------------------------------------
# Ethernet card drivers:
#
#  Driver       Bus     Description
#
#  3c503        ISA     3COM EtherLinkII (3c503)
#  3c505        ISA     3COM Etherlink Plus (3c505)
#  3c507        ISA     3COM Etherlink 16 (3c507)
#  3c509        ISA     3COM EtherLinkIII (3c509)
#  3c515        ISA     3COM EtherLink XL ISA (3c515)
#  3c59x        PCI     3COM Vortex/Boomerang 3c59x,3c900,3c905
#  8139cp       PCI     RealTek 8139C+
#  8139too      PCI     RealTek 8129/8139 10/100 MB (NEW)
#  rtl8139-db   PCI     RealTek 8129/8139, Donald Beckers Version, see 
#                       <http://www.scyld.com/network/rtl8139.html>
#  82596                Apricot Xen-II on board Ethernet
#  acenic       PCI     Alteon AceNIC Gigabit Ethernet
#  at1700       ISA     AT1700 (Fujitsu 86965) ISA
#  b44          PCI     Broadcom 4400
#  cs89x0       ISA     IBM Etherjet, cs89x0 based Cards
#                       (Option io=0xnnn necessary!)
#  de4x5        PCI/EISA Digital DE425, DE434, DE435, DE450, DE500
#  depca        ISA     DEPCA, DE10x, DE200, DE201, DE202, DE422
#  dgrs         PCI     Digi International RightSwitch PCI/EISA
#  dl2k         PCI     D-Link DL2000-based Gigabit Ethernet Adapter
#  dmfe         PCI     DM9102 compatible PCI cards from Davicom
#  e1000        PCI     Intel EtherExpress PRO/1000 Gigabit Ethernet
#  e100         PCI     Intel's original driver for EEPRO100
#  e2100        ISA     Cabletron E21xx ISA
#  eepro100     PCI     Intel EtherExpressPro PCI 10+/100B/100+
#  eepro        ISA     Intel EtherExpress Pro/10
#  eexpress     ISA     EtherExpress16 ISA
#  epic100      PCI     SMC EPIC/100 (EtherPower II) PCI
#  eth16i       ISA/EISA    ICL EtherTeam 16i/32
#  ewrk3        ISA     EtherWORKS 3 ISA (DE203, DE204, DE205)
#  fealnx       PCI     ASOUND LAN 8139 card - not RTL8139 (NEW)
#  hamachi      PCI     GNIC-II Gigabit Ethernet
#  hp100        ISA/EISA/PCI    HP 10/100VG PCLAN (ISA, EISA, PCI)
#  hp           ISA     HP PCLAN (27245, 27xxx) ISA
#  hp-plus      ISA     HP PCLAN+ (27247B and 27252A) ISA
#  lance        ISA     AMD LANCE and PCnet (AT1500, NE2100) ISA
#  lp486e               Intel Professional Workstation/panther ethernet driver
#  natsemi      PCI     National Semiconductor
#  ne2k-pci     PCI     NE2000 PCI clone (eg. Realtek 8029, Winbond 89c940)
#  ne           ISA     NE2000 ISA clone (eg. Realtek 8019,
#                       Accton 16xx, NatSemi 8390, UMC 9003/9008)
#  ni5010               MiCom-Interlan NI5010
#  ni52                 NI5210 card (i82586 Ethernet chip)
#  ni65                 ni6510 (am7990 'lance' chip)
#  ns83820      PCI     cards with National Semiconductor 83820 chip
#  pcnet32      PCI     AMD PCI PCnet32
#  r8169        PCI     Realtek 8169 Gigabit Ethernet
#  sis900       PCI     SiS 900/7016
#  sk98lin      PCI     SysKonnect Gigabit Ethernet Server Adapters
#  smc9194              SMC's 9000 series of Ethernet cards
#  smc-ultra    ISA     SMC ULTRA
#  starfire     PCI     Starfire
#  sundance     PCI     DFE-550FX or DFE-530TXS (NEW)
#  tg3          PCI     Broadcom Tigon3
#  tlan         PCI     TI ThunderLAN (Compaq Netelligent ...)
#  tulip        PCI     DECchip Tulip (dc21x4x) PCI
#  via-rhine    PCI     VIA Rhine PCI (3043, VT86c100A, dfe-530tx)
#  wd           ISA     SMC WD80*3
#  winbond-840  PCI     Winbond 840
#  sunhme       PCI/Sbus    Sun Happy Meal 10/100baseT support
#                           (only QFE is tested)
#  yellowfin    PCI     Packet Engines G-NIC PCI Gigabit Eth Adapter
#
# Donald Becker drivers, see <http://www.scyld.com/>
#
#  epic100-db
#  3c59x-db             This driver is for the 3Com "Vortex" and
#                       "Boomerang" series ethercards. Members of the
#                       series include Fast EtherLink
#                       3c590/3c592/3c595/3c597 and the EtherLink XL
#                       3c900 and 3c905 cards.
#
#
# Drivers below need the Package pcmcia installed:
#
#  3c574_cs     PCMCIA  3Com 574
#  3c589_cs     PCMCIA  3Com 589
#  axnet_cs     PCMCIA  Asix AX88190 Fast Ethernet
#  fmvj18x_cs   PCMCIA  Fujitsu FMV-J181/182 Ethernet
#  nmclan_cs    PCMCIA  New Media Ethernet LAN
#  pcnet_cs     PCMCIA  NS8390-based cards (NE2000, DLINK etc)
#  smc91c92_cs  PCMCIA  SMC91c92-based cards
#  xirc2ps_cs   PCMCIA  Xircom: CE2, CEM28, CEM33, or CE3
#
# If you don't find your Cardbus Card here then try the equivalent PCI-Driver:
# 3c59x instead of 3c575_cb or 8139too instead of realtek_cb
#
# These drivers need PCMCIA _and_ WLAN:
#
#  orinoco_cs   PCMCIA  Lucent/Orinoco WLAN-Cards
#  hostap_cs    PCMCIA  PrismII/2.5/3 based Cards - supports AP-Mode
#  wavelan_cs   PCMCIA  WaveLAN
#  wl24_cs      PCMCIA  ELSA Airlancer MC-2 - Should have Firmware 2.10
#  airo_cs      PCMCIA  Cisco Aironet 4500 & 4800 series PCMCIA cards
#  ray_cs       PCMCIA  Raylink wireless cards
#  netwave_cs   PCMCIA  Netwave AirSurfer Wireless LAN
#
# These drivers need Package WLAN
#
# WLAN-Card Drivers IEEE802.11b:
#
#  hostap_pci   PCI     Prism 2.5 based PCI Wlan Cards
#  hostap_plx   PCI     Prism 2,2.5 and 3 based PCMCIA-WLan Cards
#                       in PLX-Adapter
#  airo         PCI/ISA Cisco Aironet 4500 & 4800 series PCI/ISA cards
#
# These 3 drivers acutally only work with Prism-II Cards - alternative driver
# to hostap_*
#  orinoco_pci  PCI     Lucent/Orinoco based WLAN-Cards
#  orinoco_plx  PCI     Lucent/Orinoco based PCMCIA WLAN-Cards in PLX Adapter
#  orinoco_tmd  PCI     Lucent/Orinoco based WLAN-Cards with TMD PCI-Bridge

# WLAN-Card Drivers IEEE802.11g:
#
#  prism54      PCI/PCMCIA  Prism GT / Prism Duette / Prism Indigo Chipsets
#                           Achten Sie auf die Hinweise zum Prism54 Treiber
#                           in der WLAN Dokumentation!
#  rt2500	PCI/CARDBUS Ralink RT2500 Cards - experimental
#
# USB-WLAN Card Drivers IEEE802.11g:
#  rt2570	USB Ralink RT2570 Sticks - experimental
#
# USB-Card Drivers:
#
#  pegasus      teledat Fast Ethernet USB
#
#  kaweth       3Com 3C19250
#               ADS USB-10BT
#               ATEN USB Ethernet
#               ASANTE USB To Ethernet Adapter
#               AOX Endpoints USB Ethernet
#               Correga K.K.
#               D-Link DSB-650C and DU-E10
#               Entrega / Portgear E45
#               I-O DATA USB-ET/T
#               Jaton USB Ethernet Device Adapter
#               Kingston Technology USB Ethernet Adapter
#               Linksys USB10T
#               Mobility USB-Ethernet Adapter
#               NetGear EA-101
#               Peracom Enet and Enet2
#               Portsmith Express Ethernet Adapter
#               Shark Pocket Adapter
#               SMC 2202USB
#               Sony Vaio port extender
#  rtl8150      RTL8150-based USB-Ethernet-Cards
#  catc         Belkin F5U111
#               CATC NetMate
#               CATC NetMate II
#               smartBridges smartNIC
#
# DSL-Modems shown as Ethernetcards:
#
#  cdcether     Ericsson PipeRider (all variants)
#               Motorola (DM100 and SB4100)
#               Broadcom Cable Modem (reference design)
#               Toshiba PCX1100U and possibly other cable modems
#               Sharp Zaurus SL-5000D
#  eagle-usb    Allied Telesyn AT-AR 215
#               Sagem 250
#               Acer ADSL Surf USB
#               D-Link DSL 260i
#               Sagem 840
#               US Robotics USR9000
#               Sagem F@st 800
##
# USB-to-USB-network-cable:
#
#  usbnet       Driver for usb-to-usb networklinks
#
# Token ring drivers (see token ring mini howto on 
#     <http://www.tldp.org/docs.html#howto> and feel 
#     free to submit documention changes:
#
#  3c359
#  abyss
#  ibmtr
#  lanstreamer
#  olympic
#  smctr
#  tmsisa
#  tmspci
#
#  If you need a dummy device use 'dummy' as you NET_DRV
#  and IP_NET_%_DEV='dummy<number>' as your device
#
#------------------------------------------------------------------------------
NET_DRV_N='1'                  # number of ethernet drivers to load, usually 1
NET_DRV_1='8139too'            # 1st driver: name (e.g. NE2000 PCI clone)
NET_DRV_1_OPTION=''            # 1st driver: additional option
NET_DRV_2='ne'                 # 2nd driver: name (e.g. NE2000 ISA clone)
NET_DRV_2_OPTION='io=0x320'    # 2nd driver: additional option

#------------------------------------------------------------------------------
# Ether networks used with IP protocol:
#------------------------------------------------------------------------------
IP_NET_N='2'                   # number of IP ethernet networks, usually 1
IP_NET_1='192.168.0.2/24'      # IP address of your n'th ethernet card and
                               # netmask in CIDR (no. of set bits)
IP_NET_1_DEV='eth0'            # required: device name like ethX
IP_NET_2='192.168.1.1/24'
IP_NET_2_DEV='eth1'

#------------------------------------------------------------------------------
# Additional routes, optional
#------------------------------------------------------------------------------
IP_ROUTE_N='1'                            # number of additional routes
IP_ROUTE_1='0.0.0.0/0 192.168.0.1'        # network/netmaskbits gateway
IP_ROUTE_2='0.0.0.0/0 192.168.6.99'       # example for default-route

#------------------------------------------------------------------------------
# Packetfilter configuration; there are two styles, old and new -
# you have to choose one of them.
# 
# Please choose the new packet filter configuration, the old one is
# deprecated and only provided for compatibility reasons. During boot
# up the configuration will be translated to the new configuration,
# printed to the screen and written to bootmsg.txt to allow for an
# easy migration to the new config style.
#
# Old style packet filter config - set ORIG_FW_CONFIG='yes' to use
# this version
#------------------------------------------------------------------------------
ORIG_FW_CONFIG='no'

    #--------------------------------------------------------------------------
    # Known networks - Networks which are allowed to pass the packet
    # filter (additional restrictions may be applied via black/white
    # lists, port based filters, port forwarding opens additional holes, ...)
    #--------------------------------------------------------------------------
    MASQ_NETWORK='IP_NET_1'    # networks to masquerade (e.g. our LAN)
    ROUTE_NETWORK=''           # same as masq_network, but packets
                               # going into these networks are not
                               # masqueraded, see documentation
    TRUSTED_NETS=''            # allow free and unmasqueraded
                               # communication between these networks

    #--------------------------------------------------------------------------
    # Host based restrictions: internal hosts to allow/deny forwarding
    #
    # FORWARD_HOST_WHITE='no'  describes a black list (forbidden)
    # FORWARD_HOST_WHITE='yes' describes a white list (allowed)
    #
    # Example:
    #   FORWARD_HOST_WHITE='no' and FORWARD_HOST_N='0':
    #    -> forwarding of 0 hosts is denied
    #    -> forwarding of all hosts is allowed
    #--------------------------------------------------------------------------
    FORWARD_HOST_WHITE='no'              # 'no': black list, 'yes': white list
    FORWARD_HOST_N='0'                   # number of allowed/denied hosts
    FORWARD_HOST_1='192.168.6.5'         # optional: 1st allowed/denied host
    FORWARD_HOST_2='@client2'            # optional: 2nd allowed/denied host
    
    #--------------------------------------------------------------------------
    # Port based restrictions: ports to reject/deny forwarding 
    #--------------------------------------------------------------------------
    FORWARD_DENY_PORT_N='3'              # no. of ports to reject/deny
                                         # forwarding
    FORWARD_DENY_PORT_1='139 REJECT-TCP' # reject forwarding of netbios
    FORWARD_DENY_PORT_2='445 REJECT-TCP'
    FORWARD_DENY_PORT_3='137-138 REJECT-UDP'

    #--------------------------------------------------------------------------
    # Accept connections from outside to several ports (served ports)
    #--------------------------------------------------------------------------
    # INPUT_POLICY='REJECT'             # be nice and use reject as policy
                                        # already defined in new style
                                        # filter section
    INPUT_ACCEPT_PORT_N='0'             # no. of ports to accept from outside
    INPUT_ACCEPT_PORT_1='22 TCP'        # e.g. allow connection to ssh service

    #--------------------------------------------------------------------------
    # Logging
    #--------------------------------------------------------------------------
    PACKETFILTER_LOG='no'               # log access to rejected/denied ports

#------------------------------------------------------------------------------
# New style packet filter config - set NEW_FW_CONFIG='yes' to use this
# version
#------------------------------------------------------------------------------
NEW_FW_CONFIG='yes'                  # new style packet filter config: yes/no

    INPUT_POLICY='REJECT'            # be nice and use reject as policy
    INPUT_ACCEPT_DEF='yes'           # use default rule set
    INPUT_LOG='yes'                  # don't log anything
    INPUT_LOG_LIMIT='3/minute:5'     # log 3 events per minute; allow a
                                     # burst of 5 events
    INPUT_REJ_LIMIT='1/second:5'     # reject 1 connection per second; allow a
                                     # burst of 5 events; otherwise
                                     # drop packet
    INPUT_UDP_REJ_LIMIT='1/second:5' # reject 1 udp packet per second; allow a
                                     # burst of 5 events; otherwise drop packet
    INPUT_LIST_N='2'
    INPUT_LIST_1='IP_NET_2 ACCEPT'   # allow all hosts in the local
                                     # network access to the router
    INPUT_LIST_2='tmpl:samba DROP NOLOG' # drop (or reject) samba access
                                         # without logging, otherwise the log
                                         # file will be filled with useless
                                         # entries

    FORWARD_POLICY='REJECT'          # be nice and use reject as policy
    FORWARD_ACCEPT_DEF='yes'         # use default rule set
    FORWARD_LOG='yes'                # don't log anything
    FORWARD_LOG_LIMIT='3/minute:5'   # log 3 events per minute; allow a
                                     # burst of 5 events
    FORWARD_REJ_LIMIT='1/second:5'   # reject 1 connection per second; allow a
                                     # burst of 5 events; otherwise
                                     # drop packet
    FORWARD_UDP_REJ_LIMIT='1/second:5'  # reject 1 udp packet per second; allow
                                        # a burst of 5 events; otherwise
                                        # drop packet
    FORWARD_LIST_N='1'
    FORWARD_LIST_1='IP_NET_2 ACCEPT' # drop samba traffic if it tries
                                     # to leave the subnet
    FORWARD_LIST_2='tmpl:samba DROP' # accept everything else

    POSTROUTING_LIST_N='0'
    POSTROUTING_LIST_1='IP_NET_1 MASQUERADE'  # masquerade traffic leaving
                                              # the subnet

    PREROUTING_LIST_N='0'
    PREROUTING_LIST_1='1.2.3.4 dynamic:22 DNAT:@client2'
                                              # forward ssh connections
                                              # coming from 1.2.3.4 to client2

#------------------------------------------------------------------------------
# Simple DMZ setup for dial-up based routers -- see documentation
#------------------------------------------------------------------------------
OPT_DMZ='no'

#------------------------------------------------------------------------------
# Optional package: PORTFW
#------------------------------------------------------------------------------
PORTFW_N='0'                          # how many portforwardings to set up
PORTFW_1_TARGET='8080'                # example 1: forward ext. port 8080
PORTFW_1_NEW_TARGET='192.168.6.15:80' # ...to int. host 192.168.6.15 port 80
PORTFW_1_PROTOCOL='tcp'               # ...using tcp
PORTFW_2_TARGET='3000-3010'           # example 2: forward portrange 3000-3010
PORTFW_2_NEW_TARGET='192.168.6.15'    # ...to int. host 192.168.6.15
PORTFW_2_PROTOCOL='tcp'               # ...using tcp

#------------------------------------------------------------------------------
# Masq modules
#------------------------------------------------------------------------------
MASQ_MODULE_N='0'                     # load n masq modules (default: only ftp)
MASQ_MODULE_1='ftp'                   # ftp
MASQ_MODULE_1_OPTION=''               # options, see documentation
MASQ_MODULE_2='irc'                   # irc
MASQ_MODULE_2_OPTION=''               # options, see documentation

#------------------------------------------------------------------------------
# Domain configuration:
#------------------------------------------------------------------------------
DOMAIN_NAME='lan.fli4l'               # your domain name
DNS_FORWARDERS='192.168.0.1'          # DNS servers of your provider,
                                      # e.g. ns.n-ix.net

OPT_DNS='yes'                         # start dns server: yes or no
    DNS_TRIGGER_DIAL_IN='no'	      # trigger a dial-in before
                                      # forwarding requests
    DNS_LISTENIP_N='0'                # if 0 then listen on all interfaces
    DNS_LISTENIP_1='IP_NET_1_IPADDR'  # first IP to listen on
    DNS_VERBOSE='yes'                 # log queries into syslog
    DNS_MX_SERVER=''                  # fqdn of the mx for your DOMAIN
    DNS_FORBIDDEN_N='0'               # number of forbidden domains
    DNS_FORBIDDEN_1='foo.bar'         # 1st forbidden domain
    DNS_FORBIDDEN_2='bar.foo'         # 2nd forbidden domain
    DNS_REDIRECT_N='0'                # number of redirected domains
    DNS_REDIRECT_1='foo.bar.foo'      # 1st redirected domain
    DNS_REDIRECT_1_IP='192.168.6.100' # IP of redirected domain
    DNS_BOGUS_PRIV='yes'              # fake reverse lookups for RFC1918
                                      # private address ranges
    DNS_FILTERWIN2K='yes'             # filters useless windows-originated DNS
                                      # requests and blocks all SRV requests

    # Special DNS configuration
    #--------------------------
    DNS_SPECIAL_N='0'                           # number of special 
                                                # dns servers, normally 0
    #DNS_SPECIAL_1='firma.de 192.168.1.12'      # 1st special dns server
                                                # for firma.de
    #DNS_SPECIAL_2='lan.firma.de 192.168.2.12'  # 2nd special dns server
                                                # for lan.firma.de

HOSTS_N='10'

HOST_1_NAME='fli4l'
HOST_1_IP='192.168.1.1'
HOST_1_MAC='00:1e:58:ec:0b:47'
HOST_2_NAME='Thomas-Janssen-Windows'
HOST_2_IP='192.168.1.10'
HOST_2_MAC='00:c1:26:0d:4f:9f'
HOST_3_NAME='Johann-Janssen'
HOST_3_IP='192.168.1.11'
HOST_3_MAC='00:08:a1:66:88:5a'
HOST_4_NAME='Thomas-Janssen-MacMini'
HOST_4_IP='192.168.1.12'
HOST_4_MAC='40:6c:8f:27:b7:d8'
HOST_5_NAME='Christa-Janssen'
HOST_5_IP='192.168.1.13'
HOST_5_MAC='00:19:21:22:c6:44'
HOST_6_NAME='Nielsen-Scanner'
HOST_6_IP='192.168.1.14'
HOST_6_MAC='00:d0:17:c0:33:bc'
HOST_7_NAME='MacBook'
HOST_7_IP='192.168.1.15'
HOST_7_MAC='00:1f:5b:ed:64:3e'
HOST_8_NAME='SamKnows-Whitebox'
HOST_8_IP='192.168.1.16'
HOST_8_MAC='f4:ec:38:f1:0c:c2'
HOST_9_NAME='iTunes'
HOST_9_IP='192.168.1.17'
HOST_9_MAC='40:6c:8f:27:ae:4f'
HOST_10_NAME='Samsung-SMT-G3210-Dachboden'
HOST_10_IP='192.168.1.18'
HOST_10_MAC='00:16:32:87:9c:b5'


#------------------------------------------------------------------------------
# DNSMASQ-DHCP server
#------------------------------------------------------------------------------
OPT_DNSDHCP='yes'                     # activate DHCP server: yes or no

    DNSDHCP_LS_TIME_DYN='3600'        # default time for dynamic leases: 1 hour
    DNSDHCP_MAX_LS_TIME_DYN='7200'    # max time  for dynamic leases: 2 hours
    DNSDHCP_LS_TIME_FIX='86400'       # default time for fix leases: 1 day
    DNSDHCP_MAX_LS_TIME_FIX='604800'  # max time for fix leases: 1 week
    DNSDHCP_LEASES_DIR='/boot'        # don't touch this until you
                                      # have read the manual!

    DNSDHCP_WINSSERVER_1=''           # IP-address of 1st external wins-server
                                      # (don't use if OPT_NMBD='yes'!)
    DNSDHCP_WINSSERVER_2=''           # IP-address of 2nd external wins-server
                                      # (don't use if OPT_NMBD='yes'!)

    # Parameters for local Networks
    # -----------------------------
    DNSDHCP_RANGE_2_START='192.168.1.100'     # start-IP of n'th ethernet,
                                              # see IP_NET_N
    DNSDHCP_RANGE_2_END='192.168.1.150'       # end-IP of n'th ethernet,
                                              # see IP_NET_N
    DNSDHCP_RANGE_2_DNS_SERVER=''             # if empty the IP of interface
                                              # IP_NET_N is used;
                                              # if set to 'none' no
                                              # dns-server is transmitted
    DNSDHCP_RANGE_2_NTP_SERVER=''             # if empty and OPT_CHRONY='yes'
                                              # the IP of interface IP_NET_N
                                              # is used; if set to 'none' no
                                              # ntp-server is transmitted
    DNSDHCP_RANGE_2_GATEWAY=''                # if empty the IP of interface
                                              # IP_NET_N is used;
                                              # if set to 'none' no
                                              # gateway is transmitted

    # Parameters for extra Networks (via relay)
    # -----------------------------------------
    DNSDHCP_EXTRA_RANGE_N='0'                    # number of extra ranges
    DNSDHCP_EXTRA_RANGE_1_START='192.168.8.2'    # start-IP of n'th extra range
    DNSDHCP_EXTRA_RANGE_1_END='192.168.8.50'     # end-IP of n'th extra range
    DNSDHCP_EXTRA_RANGE_1_NETMASK='255.255.255.0'  # netmask for extra range
    DNSDHCP_EXTRA_RANGE_1_DNS_SERVER='192.168.8.1' # DNS Server for extra range
    DNSDHCP_EXTRA_RANGE_1_NTP_SERVER=''          # NTP Server for extra range
    DNSDHCP_EXTRA_RANGE_1_GATEWAY='192.168.8.1'  # default gateway for
                                                 # extra range

    DNSDHCP_EXTRA_RANGE_1_DEVICE='eth0'    # device used to reach extra network
                                                   

    # Deny hosts from dhcp-Access
    # ---------------------------
    DNSDHCP_DENY_MAC_N='0'                    # number of denied MAC addresses
    DNSDHCP_DENY_MAC_1='00:01:02:03:04:05'    # MAC address is denied from DHCP


#------------------------------------------------------------------------------
# imond configuration:
#------------------------------------------------------------------------------
START_IMOND='no'                    # start imond: yes or no
    IMOND_USE_ORIG='yes'            # use the original version of imond instead
                                    # of the development version: yes or no
    IMOND_PORT='5000'               # port (tcp), don't open it to the outside
    IMOND_PASS=''                   # imond-password, may be empty
    IMOND_ADMIN_PASS=''             # imond-admin-password, may be empty
    IMOND_LED=''                    # tty for led: com1 - com4 or empty
    IMOND_BEEP='no'                 # beep if connection going up/down
    IMOND_LOG='no'                  # log /var/log/imond.log: yes or no
    IMOND_LOGDIR='/var/log'         # log-directory, e.g. /var/log
    IMOND_ENABLE='yes'              # accept "enable/disable" commands
    IMOND_DIAL='yes'                # accept "dial/hangup" commands
    IMOND_ROUTE='yes'               # accept "route" command
    IMOND_REBOOT='yes'              # accept "reboot" command

#------------------------------------------------------------------------------
# Generic circuit configuration:
#------------------------------------------------------------------------------
IP_DYN_ADDR='yes'                   # use dyn. IP addresses (most providers do)
DIALMODE='auto'                     # standard dialmode: auto, manual, or off

#------------------------------------------------------------------------------
# optional package: syslogd
#------------------------------------------------------------------------------
OPT_SYSLOGD='yes'                      # start syslogd: yes or no
    SYSLOGD_DEST_N='1'                 # number of destinations
    SYSLOGD_DEST_1='*.* /data/log/messages.log'  # n'th prio & destination of syslog msgs
    SYSLOGD_DEST_2='*.* /dev/console'  # example: loghost 192.168.6.2
    SYSLOGD_DEST_3='kern.info /var/log/dial.log'  # example: log infos to file

#------------------------------------------------------------------------------
# Optional package: klogd
#------------------------------------------------------------------------------
OPT_KLOGD='yes'                     # start klogd: yes or no

#------------------------------------------------------------------------------
# Optional package: y2k correction
#------------------------------------------------------------------------------
OPT_Y2K='yes'                       # y2k correction: yes or no
    Y2K_DAYS='0'                    # correct hardware y2k-bug: add x days

#------------------------------------------------------------------------------
# Optional package: PNP
#------------------------------------------------------------------------------
OPT_PNP='no'                        # install isapnp tools: yes or no
