##-----------------------------------------------------------------------------
## hd.txt - fli4l configuration parameters                         3.0.1
##
##        P L E A S E   R E A D   T H E   D O C U M E N T A T I O N ,
##                      S E E   R E A D M E . T X T
##
##        B I T T E  U N B E D I N G T   D I E   D O K U M E N T A T I O N
##              L E S E N ,  S I E H E   R E A D M E . T X T
##
## Creation:     26.06.2001  fm
## Last Update:  $Id: hd.txt 10738 2005-12-26 12:36:58Z arwin $
##
## Copyright (c) 2001 - 2005 Frank Meyer <frank@fli4l.de>
##
## This program is free software; you can redistribute it and/or modify
## it under the terms of the GNU General Public License as published by
## the Free Software Foundation; either version 2 of the License, or
## (at your option) any later version.
##-----------------------------------------------------------------------------

#------------------------------------------------------------------------------
# Optional package: HD controler drivers
#
#  Driver       Bus     Description
#
#  ide-hd               generic IDE-Controllers, NOT IDE-Raid
#  ide-floppy           LS-120 and ATAPI-Zip, try this one or ide-hd
#  atp870u      PCI     ACARD 870U/W 
#  aha152x      ISA/VLB Adaptec AHA-1510, AHA-1520, AHA-1522, and AHA-2825
#  aha1542      ISA     Adaptec AHA154x Controller
#  aic7xxx      PCI     various aic7xxx based Adaptec SCSI controllers but
#                       *not* AHA2920
#  advansys             all adapters manufactered by Advansys
#  buslogic     PCI     BusLogic MultiMaster and FlashPoint adapters
#  fdomain      PCI     Future Domain 16xx SCSI/AHA-2920A
#  g_ncr5380    ISA     generic NCR family of SCSI controllers
#  initio       PCI     Initio 91XXU(W) SCSI host adapter
#  a100u2w      PCI     Initio INI-A100U2W SCSI host adapter
#  sym53c8xx_2  PCI     All Adapter with Symbios Logic (LSI) Chips 53c8xx
#  ncr53c8xx    PCI     NCR53C8XX family of PCI-SCSI controllers
#  sim710               Simple 53c710 SCSI support (Compaq, NCR machines)
#  sym53c416    ISA     sym53c416 SCSI host adapter
#  tmscsim      PCI     Tekram DC390(T) and Am53/79C974 based adapters
#  ultrastor            UltraStor 14F, 24F and 34F SCSI-2
#
# This is an Industry Standard Flash-Module:
#
#  diskonchip           M-Sys DiskOnChip
#
# Some drivers for CDROM-Drives:
#  ide-cd               IDE-CDROM
#  scsi-cd              SCSI-CDROM, you need to select a SCSI-Driver too!
#
#------------------------------------------------------------------------------
OPT_HDDRV='yes'                 # install drivers for harddisk: yes or no
HDDRV_N='2'                     # number of HD drivers to load, usually 1
HDDRV_1='ide-hd'                # 1st driver: name (e.g. ide-hd)
HDDRV_1_OPTION=''               # 1st driver: additional option
HDDRV_2='ide-cd'
HDDRV_2_OPTION=''

#------------------------------------------------------------------------------
# Optional package: install on HD or Flashdisk
#------------------------------------------------------------------------------
OPT_HDINSTALL='no'              # install on harddisk: yes or no
HDINSTALL_RECOVERYTIME='60'     # timeout for recovery-installation in seconds

#------------------------------------------------------------------------------
# Optional: mount additional devices
#------------------------------------------------------------------------------
OPT_MOUNT='yes'                 # mount partitions, created by opt_hdinstall

#------------------------------------------------------------------------------
# Optional package: Power-Down for IDE Harddisk
#------------------------------------------------------------------------------
OPT_HDSLEEP='no'                # power down HD after some time
HDSLEEP_TIMEOUT='2'             # wait 2 minutes until power down
