# 9.2 Tokenring - Auszug aus Configure.help des Linux-Kernels

    Token Ring driver support
    CONFIG_TR
      Token Ring is IBM's way of communication on a local network; the
      rest of the world uses Ethernet. To participate on a Token Ring
      network, you need a special Token ring network card. If you are
      connected to such a Token Ring network and want to use your Token
      Ring card under Linux, say Y here and to the driver for your
      particular card below and read the Token-Ring mini-HOWTO, available
      from <http://www.tldp.org/docs.html#howto>. Most people can
      say N here.

    IBM Tropic chipset based adapter support
    CONFIG_IBMTR
      This is support for all IBM Token Ring cards that don't use DMA. If
      you have such a beast, say Y and read the Token-Ring mini-HOWTO,
      available from <http://www.tldp.org/docs.html#howto>.

      Warning: this driver will almost definitely fail if more than one
      active Token Ring card is present.

      This driver is also available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called ibmtr.o. If you want to compile it as a
      module, say M here and read <file:Documentation/modules.txt>.

    IBM Olympic chipset PCI adapter support
    CONFIG_IBMOL
      This is support for all non-Lanstreamer IBM PCI Token Ring Cards.
      Specifically this is all IBM PCI, PCI Wake On Lan, PCI II, PCI II
      Wake On Lan, and PCI 100/16/4 adapters.

      If you have such an adapter, say Y and read the Token-Ring
      mini-HOWTO, available from <http://www.tldp.org/docs.html#howto>.

      This driver is also available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called olympic.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

      Also read <file:Documentation/networking/olympic.txt> or check the
      Linux Token Ring Project site for the latest information at
      <http://www.linuxtr.net/>.

    IBM Lanstreamer chipset PCI adapter support
    CONFIG_IBMLS
      This is support for IBM Lanstreamer PCI Token Ring Cards.

      If you have such an adapter, say Y and read the Token-Ring
      mini-HOWTO, available from <http://www.tldp.org/docs.html#howto>.

      This driver is also available as a modules ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The modules will be called lanstreamer.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.
    Generic TMS380 Token Ring ISA/PCI/MCA/EISA adapter support
    CONFIG_TMS380TR
      This driver provides generic support for token ring adapters
      based on the Texas Instruments TMS380 series chipsets.  This
      includes the SysKonnect TR4/16(+) ISA (SK-4190), SysKonnect
      TR4/16(+) PCI (SK-4590), SysKonnect TR4/16 PCI (SK-4591),
      Compaq 4/16 PCI, Thomas-Conrad TC4048 4/16 PCI, and several
      Madge adapters.  If you say Y here, you will be asked to select
      which cards to support below.  If you're using modules, each
      class of card will be supported by a separate module.

      If you have such an adapter and would like to use it, say Y and
      read the Token-Ring mini-HOWTO, available from
      <http://www.tldp.org/docs.html#howto>.

      Also read the file <file:Documentation/networking/tms380tr.txt> or
      check <http://www.auk.cx/tms380tr/>.

      This driver is also available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called tms380tr.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

    Generic TMS380 PCI support
    CONFIG_TMSPCI
      This tms380 module supports generic TMS380-based PCI cards.

      These cards are known to work:
         - Compaq 4/16 TR PCI
         - SysKonnect TR4/16 PCI (SK-4590/SK-4591)
         - Thomas-Conrad TC4048 PCI 4/16
         - 3Com Token Link Velocity

      This driver is available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called tmspci.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

    Generic TMS380 ISA support
    CONFIG_TMSISA
      This tms380 module supports generic TMS380-based ISA cards.

      These cards are known to work:
         - SysKonnect TR4/16 ISA (SK-4190)

      This driver is available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called tmsisa.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

    Madge Smart 16/4 PCI Mk2 support
    CONFIG_ABYSS
      This tms380 module supports the Madge Smart 16/4 PCI Mk2
      cards (51-02).

      This driver is available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called abyss.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

    SMC ISA/MCA Token Ring adapter support
    CONFIG_SMCTR
      This is support for the ISA and MCA SMC Token Ring cards,
      specifically SMC TokenCard Elite (8115T) and SMC TokenCard Elite/A
      (8115T/A) adapters.

      If you have such an adapter and would like to use it, say Y or M and
      read the Token-Ring mini-HOWTO, available from
      <http://www.tldp.org/docs.html#howto> and the file
      <file:Documentation/networking/smctr.txt>.

      This driver is also available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will be called smctr.o. If you want to compile it
      as a module, say M here and read <file:Documentation/modules.txt>.

    3COM 3C359 Token Link Velocity XL PCI adapter support
    CONFIG_3C359
      This is support for the 3Com PCI Velocity XL cards, specifically
      the 3Com 3C359, please note this is not for the 3C339 cards, you
      should use the tms380 driver instead.

      If you have such an adapter, say Y and read the Token-Ring
      mini-HOWTO, available from <http://www.tldp.org/docs.html#howto>.

      This driver is also available as a module ( = code which can be
      inserted in and removed from the running kernel whenever you want).
      The module will will be called 3c359.o. If you want to compile it
      as a module, say M here and read Documentation/modules.txt.

      Also read the file <file:Documentation/networking/3c359.txt> or check the
      Linux Token Ring Project site for the latest information at
      <http://www.linuxtr.net>

Das Fli4l-Team
23. Februar 2006