fli4l documentation - Configuration

2. Basic configuration - General circuit configuration

##### :::[ IP_DYN_ADDR ][ DIALMODE ]:::

#### IP_DYN_ADDR

If you use a connection with dynamic addresses, you will have to set IP_DYN_ADDR to 'yes'. If you will have static IP addresses, you will use value 'no'. Most internet providers use dynamic addresses.

Default setting: IP_DYN_ADDR='yes'

##### [ top ]

#### DIALMODE

The default dial mode of FLI4L is: 'auto'. That means, there will be automatic dialing when you call an IP address outside your own network (IP address range). Additionally it is possible to define your dial mode as 'manual' or 'off' . If you did so, you will have to use the client imonc for dialing anywhere.

Default setting: DIALMODE='auto'

##### [ top ]