README

		      Welcome to CMD QuickIDE   
		      -----------------------

  This README file contains important information about QuickIDE
  and your CMD 32-Bit Local Bus IDE Controller.  For the latest 
  information about your CMD IDE controller and QuickIDE, please read 
  this file in its entirety.

  This is the general release of CMD CSA-6460 32-bit local bus drivers. 
  This release includes the following drivers :

  - DOS driver 
  - OS/2 2.x driver             
  - Windows NT 3.1 driver
  - Windows NT 3.5 driver
  - SCO Unix 3.2.4 driver
  - Netware 3.1x driver
  - Netware 4.xx driver


NOTE:  Some IDE drives have firmware bugs which cause them to declare
       themselves as Mode 2 drives even though they are really slower.
       As a result, the following exception table has been implemented in
       all CMD drivers:

      1. Samsung Mode 2 drives are slowed down to Mode 1.
      2. Maxtor Mode 2 drives are slowed down to Mode 1.
      3. Quantum Mode 2 drives are slowed down to Mode 0.

      If you have a drive with a similar bug not listed above, refer to
      the following command line switches:
      1) DOS: CMD646X.SYS - /O - documented in README.DOS
      2) OS/2: CMD646X.ADD - /PIOMODE:d - documented in README.OS2
      3) NT: see README.NT - ATA PIO Mode Timing Overrides


INSTALLATION
------------

  Software Drivers:
     DOS: see install procedure below
     NetWare 3.1x   : see install procedure below, additional info
		      in NETWARE.3X\README.NW3
     NetWare 4.xx   : see NETWARE.4X\README.NW4
     OS/2 Warp 2.x  : see OS2WARP\README.OS2
     Windows 3.1x   : see WINDOWS\README.WIN
     Windows NT 3.1 : copy the files in NT31 directory to root directory of
                      diskette before installation and see NT31\README.NT
     Windows NT 3.5 : copy the files in NT35 directory to root directory of
                      diskette before installation and see NT35\README.NT
     SCO UNIX 3.2.x : see SCO\README.SCO

  Connect your IDE drives to your CMD IDE controller.  Make sure that 
  the jumpers on the drives are set correctly for Master and Slave 
  drives.  If your CMD IDE controller is on an add-in card, plug it
  into a suitable Local Bus slot.

  Next, configure your CMOS with the proper drive types for the
  drive(s) connected to the IDE port.  If you are not sure
  of the drive type(s) and your BIOS does not auto-detect, you can
  use CheckIDE:

     1) Configure your CMOS for NO hard disks
     2) Boot your system with a floppy disk, and then replace the
	boot floppy with the QuickIDE floppy.
     3) Run "checkide" and make note of the drive geometry (heads,
	sectors,cylinders).
     4) Configure your CMOS user drive type and the geometry
	information from step (3).  Set the landing zone equal to
	the number of cylinders minus 1, and the write precompensation
	cylinder to 65535.

  Install the desired operating system that you are going to use on your 
  hard drive.
  
  Next, you must install the QuickIDE software for DOS and NetWare 3.1x. 
  For OS/2, NetWare 4.x, and SCO Unix, refer to README.OS2, README.NW, 
  and README.SCO, respectively.  For Windows NT 3.1 or NT 3.5, copy the 
  files under NT31 or NT35 directory to root directory of diskette before 
  installation.  To start QuickIDE installation, type the path where your 
  installation program resides.  For instance, if you will be installing 
  from drive A, type:

    A:INSTALL

  Once QuickIDE Installation loads, you will be guided through
  the installation process with a series of prompts and dialogs.
  If you have a mouse, be sure to load your mouse driver first.
  If you do not have a mouse, the keyboard will work fine.  The
  following key definitions may be helpful:

    ARROW KEYS - move within a field.
    TAB - move from one field to another within a window or dialog
   
  To select a button or menu, hold down ALT while pressing the
  underlined letter in the button or menu.

  After you have answered all the questions, QuickIDE will copy
  files to your C: drive and perform edits to files as needed.
  Backup copies of any files it changes will be created in case you
  want to undo the installation.  The files which may be modified are:
  CONFIG.SYS and  AUTOEXEC.BAT.  The original files will be renamed to
  CONFIG.000, etc.


