
                    AT&T UNIX

The AT&T driver is found on the SCO/ISC/AT&T UNIX diskette.

<DRIVER INSTALLATION>

To install the driver, insert the working copy of the UNIX driver diskette in
drive A.

A) At the prompt, type

        installpkg

B) type "f" to install from floppy drive

C) press <Enter> to install the driver

D) press <Enter> to choose the AT&T UNIX is being installed

E) press <Enter> to reboot the system


<DRIVER LISTING>

To ensure the driver is installed, type

        displaypkg


<DRIVER REMOVAL>

To remove the driver,

A) At the prompt, type

        removepkg

B) type the corresponding number of:

   "IDE32C Cache Controller Driver Package"

C) press <Enter> to remove IDE32C driver

D) press <Enter> to reboot
