      * * * WINDOWS 95 DRIVER FOR DC-690CD CACHE CONTROLLER * * *

Due to the nature of Plug & Play, the Windows 95 Driver (DC690.PDR) can only
support one DC-690CD as the Primary IDE card. If you are using 1 or 2
DC-690CDs in the same system with the ATAPI port(s) disabled, use the driver
for the other DC-600 Series cards (DC6X0.PDR) in the directory: \WIN95\OTHERS.

1. This driver is only for the DC-690CD, NOT the DC-690, DC-690B or DC-690C.
   For other DC-690 models, use the driver in the \WIN95\OTHERS directory.

2. The Drive_Type in your system CMOS must be on Type_1. If the drive type
   is set for "Not Installed" there may be problems getting the system to run
   in 32-Bit mode under Windows 95.

I. Windows 95 Driver Installation 

   1. Boot Windows 95 and click on "Start"
   2. Select "RUN"
   3. Type "A:\WIN95\DC690CD\INSTALL.EXE" (Where A:\WIN95\DC690CD is the path
      to the Tekram WIN95 driver)
   4. Click "Next"
   5. Select NO to bypass the Search for New Hardware, and Click "Next"
   6. Select "Hard disk controllers" from the list
   7. Click "Next"
   8. Click "Have disk"
   9. Type "A:\WIN95\DC690CD"
  10. The "Tekram IDE Cache Controller (DC6X0-CD(F))" should be highlighted.
  11. Click "Next", Click "Next"
  12. The message  "To finish setting up your new device driver you must
      restart your computer. do you want to restart your computer now?"
      will then appear. Click on "YES" to restart the system.

[Note1]
   After Windows 95 reboots, it will detect the DC-690CD as a new Primary PCI
   IDE controller and ask if you would like to restart. Select "NO". The
   system will then detect the Secondary IDE controller and ask to restart.
   At this point choose "YES".

[Note2]
   There should be three controllers under the Device Manager in Windows 95
   after the install:
        1. DC-690 Primary IDE Controller (dual fifo)
        2. DC-690 Secondary IDE Controller (dual fifo)
        3. Tekram PCI IDE Cache Controller (DC690-CD)
                
[Note3]
   Keep in mind that if your system board has an on-board controller, it
   will probably show up in the Device Manager with an exclamation. THIS IS
   NORMAL. When opened, this device should read "Disabled in the Hardware".

II. Windows 95 Driver Uninstallation

   1. Click on "Start"
   2. Select "RUN"
   3. Type "A:\WIN95\DC690CD\UNINSTAL"
   4. The message  "To finish un-installation you must restart your computer,
      do you want to restart your computer now?" will appear. Click "YES"
      to restart the system.

