;DrIvEr DeScRiPtIoN

SyntaxVersion: 1.00

	;file: concatenated to IDENV40.DSK

	Driver IDENV40_DESCR
	{
		Description:					"Netware 4.0x 32 bits Device Driver For IDE Cache Controller"

		Help:						"Use this driver with 32 bits IDE cache controller
								 with firmware version 2.00 and above : This driver
								 can use controllers at both the primary and the
								 secondary addresses.  This allows two adapter
								 cards to be installed in the host bus.  Load the
								 device driver once for each adapter card.\n\n

								 The default options are for the primary
								 adapter address settings.  This is the
								 standard controller.  If a second
								 adapter is inserted, use another option."


		ParameterVersion:			1.00
		File:						IDENV40.DSK


		PROMPT INT REQ
		{
			Values: 				E, F
			Default:				E
			ReservedLength: 			1
		}

		PROMPT PORT REQ
		{
			Values: 				170, 1F0
			Default:				1F0
			ReservedLength: 			3
		}

;		LIST ParameterStamp
;		{
;			Description:			"Look for NetWare Ready Stamp or CCM stamp  on the disk"
;
;			Help:				"Use this option to cause the driver to look for a NetWare Ready or
;							CCM stamp on the disk and then use the disk parameters from that stamp
;							instead of using the parameters found in the system BIOS.  Use this
;							option only if there is a stamp on the disk."
;
;			CDescription:		"No"
;			Choice: 				''
;
;			CDescription:		"Yes"
;			Choice: 				'/n'
;
;			Default:				1
;			OutputFormat:			'%s'
;		}

;		LIST ReadRedirectedBIOS
;		{
;			Description:	"Allow BIOS redirection on secondary controller"
;
;			Help:			"Use this option if you have drives that the driver
;							is not seeing on a secondary controller.\n
;							*** WARNING*** This option can cause incorrect drive
;							registration if the BIOS table is not complete."
;
;			CDescription:		"No"
;			Choice: 			''
;
;			CDescription:		"Yes"
;			Choice: 			'/l'
;
;			Default:			1
;			OutputFormat:		'%s'
;		}
;
	}

;DrIvEr DeScRiPtIoN EnD


