* * * WINDOWS 95 DRIVER FOR ALL TEKRAM CACHE CONTROLLERS EXCEPT DC-690CD * * *
                       
This Tekram Windows 95 Driver (DC6X0.PDR) supports the following IDE Caching
Controllers: DC-600CD/600CF/600C, DC-620B, DC-680T/C/CD, DC-690B/C
*BIOS/FIRMWARE must be version 2.0 or higher

[Note1]: The DC-690CD uses the driver in the \WIN95\DC690CD directory.
         *Unless you are using 1 or 2 DC-690CDs in the same system with the
         ATAPI port(s) disabled, in which case this driver \WIN95\OTHERS
         is the correct driver to use...
[Note2]: The DC-690C should have JP3 set to pins 1-2 for proper operation.
[Note3]: The drive type in CMOS setup should be set to "Type 1".

Installation instuctions:

I. 1st time installation

  1.  Install Windows 95
  2.  Double-click the SYSTEM icon in the Control Panel. Remove the "Standard
      IDE Controller(s)" from the Device Manager. Exit System Properties. 
  3.  Open the Control Panel and Double-Click the "Add New Hardware" icon.
  4.  Click "Next".
  5.  Choose NO to bypass Searching for New Hardware.
  6.  Choose Hard Disk Controllers from the list and then click "Next".
  7.  Click "Have Disk".
  8.  Enter A:\WIN95\OTHERS or the path to the Tekram Windows 95 driver
      and click O.K.
  9.  The "Tekram IDE Cache Controller (DC6X0-CD(F))" should be highlighted.
 10.  Click "Next", Click "Next".
 11.  Click "Finish".
 12.  Restart the system.

*To install a Secondary Tekram Controller, repeat steps 3-12.

====> After rebooting:
   Check the Hard Disk Controller(s) in Device Manager to see if there are
   any exclamation points. If there are, check the resources. The primary
   controller should be using Interrupt 14. Make sure it is not using 15.
   If it is, change the configuration under "Resources" to
   "Basic Configuration 0". If there is a secondary card installed, that
   should be using INT 15 (Basic Configuration 1).

II. Driver update

  1.  Enter "Device Manager".
  2.  Select "Hard disk controllers".
  3.  Double-Click the "Tekram IDE Cache Controller(DC6X0-CD(F))".
  4.  Click the Driver Tab.
  5.  Click "Change driver".
  6.  Click "Have disk".
  7.  Type: "A:\WIN95\OTHERS" (Or the directory containing the Tekram Driver)
  8.  The "Tekram IDE Cache Controller (DC6X0-CD(F))" should be highlighted.
  9.  Click on "OK".
 10.  Restart the system.
