This README file covers the driver installation and removal procedures
for Windows 3.1x and WFW v3.11.

The Tekram WIN31X driver is designed to allow 32-bit-bus EISA/VL/PCI IDE
caching controllers to use WIN31 32-Bit Disk Access.

Windows 3.1x or Windows for WorkGroups 3.11 must be installed before
beginning these procedures.

(A). Driver Installation:
        1. Execute the program "\WINDRV\INSTALL.EXE" from the floppy drive

        or

        2. Enter Windows and run the same file "\WINDRV\INSTALL.EXE"

(C). Driver Removal:
        1. During the driver installtion, the original SYSTEM.INI under your
           Windows directory will be renamed to SYSTEM.001. Rename SYSTEM.001
           back to SYSTEM.INI and the driver will be removed.
