[Version]
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%HIGHPOINT%
;CatalogFile=
DriverVer=06/18/2000,1.0.0.06182000

; Class Install
[ClassInstall32.NT]
Addreg=SCSIReg

[SCSIReg]
HKR,,,,%SCSIClassName%
HKR,,Installer32,,"SysSetup.Dll,ScsiClassInstaller"
HKR,,Icon,,"-10"
HKR,,LegacyInfOption,,"SCSI"

[DestinationDirs]
DefaultDestDir  = 12 ; DIRID_DRIVERS

[ControlFlags]
;
; Exclude the following devices from Select Device list.
; These represent 'combination' driver nodes, for which there are separate items to be
; presented to the user.  These combination nodes are only used when figuring out what
; driver node to associate with a pre-existing service.
;
[Manufacturer]
%Highpoint%=Highpoint

[NODRV]
;
; The empty service entry is to fool the class installer - without a service
; entry this install section would be rejected as being part of a win9x inf.
; 

[NODRV.Services]
NoDriver=1

[Highpoint]
%hpt3xx.DeviceDesc%			 =Hpt3xxPCI,HPT3XX_SCSI

[Hpt3xxPCI.NT]
CopyFiles=@Hpt3xxNT.sys
Reboot

[Hpt3xxPCI.NT.Services]
AddService = Hpt3xxNT, %SPSVCINST_ASSOCSERVICE%, Hpt3xxPCI_Service_Inst, Miniport_EventLog_Inst

[Hpt3xxPCI_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\Hpt3xxNT.sys
LoadOrderGroup = SCSI Miniport

;*************************************************************
;These addreg sections should be used when installins services to indicate
;which interface types are safe for PNP and which aren't.  INTERFACE_TYPE
;is defined in NTDDK.H

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[pnpsafe_isa_addreg]
HKR, "Parameters\PnpInterface", "1", 0x00010001, 0x00000001

[pnpsafe_eisa_addreg]
HKR, "Parameters\PnpInterface", "2", 0x00010001, 0x00000001

[pnpsafe_mca_addreg]
HKR, "Parameters\PnpInterface", "3", 0x00010001, 0x00000001

[cardbus_interface_type]
HKR, "ScsiPort", "LegacyInterfaceType", 0x00010001, 0x00000005

;*************************************************************
;The EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[SourceDisksNames]
1 = "HPT370 UDMA/ATA100 RAID Driver Diskette",\disk1,,,
2 = "HPT370 UDMA/ATA100 RAID Driver Diskette",\disk1,,\WIN
3 = "HPT370 UDMA/ATA100 RAID Driver Diskette",\disk1,,\NT
4 = "HPT370 UDMA/ATA100 RAID Driver Diskette",\disk1,,\2K

[SourceDisksFiles]
Hpt3xxNT.inf = 1,,
Hpt3xxNT.sys = 1,,

[strings]
Highpoint="Highpoint"
hpt3xx.DeviceDesc                      ="HPT370 UDMA/ATA100 RAID Controller"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
