CMD PCI646X 32-Bit Local Bus IDE Driver for Netware
---------------------------------------------------

The CMD C646X4X hard disk driver can be run on Netware 4.X. It supports up 
to 2 IDE channels. 

Note that the CMD 32-Bit Local-Bus IDE driver for DOS has to be loaded in 
CONFIG.SYS in order for the C646X4X Netware driver to function properly.

The C646X4X driver will inherit the drive mode and timing setting from DOS
driver.  There is no option to specify for this driver.  It will automatically
look for all the drives on the IDE channel(s).


INSTALLATION
------------

1) Install Netware 4.X

2) When installation of Netware 4.X prompts for hard disk driver name, specify
   the full path name of the CMD Netware driver. For example, if the CMD
   installation diskette is in drive A, you can specify

	A:\NETWARE.4X

3) Select C646X4X

4) Proceed with the rest of the Netware installation.
