This README file explains the Driver Installation and Removal.

(A). Please be advised that this driver diskette works for ISA/EISA/VL/PCI
IDE caching controllers.


(B). Driver Installation:
     1. Insert the driver diskette into Floppy Drive A:

     2. Under OS/2 V2.X/Warp 3.0 install the driver by keying the following
        command:

        [C:\] ddinstal

        This command copies the file, OS2_32.ADD, from driver diskette to
        C:\OS2 directory. The old CONFIG.SYS will be re-named as CONFIG.1,
        which also resides in the C:\ directory.

     3. Re-boot the system

(C). Driver Removal:
     1. During the driver installation, the original CONFIG.SYS under your
        C:\ directory will be renamed as CONFIG.1. Rename CONFIG.1 back to
        CONFIG.SYS, you'll have the driver removed.

           [C:\] COPY CONFIG.1 CONFIG.SYS

     2. Re-boot the system


Note !!!
  1. For OS/2 Warp 3.x ATAPI CD-ROM driver C:\OS2\BOOT\IBMIDECD.FLT
     date code later than 10-06-94, if an ATAPI CD-ROM drive was
     installed as Master drive at 2nd IDE port and no slave drive at 2nd IDE
     port, then must add the command line option "/master" as follow:

        BASEDEV=OS2_32.ADD /master
