
                    SCO UNIX

The SCO driver is located on the SCO/ISC/AT&T UNIX diskette.

<DRIVER INSTALLATION>

To install the driver, insert the working copy of the UNIX driver diskette in
drive A.

A.1) For SCO 3.2v2

     To prepare the installation for 360KB (5"1/4) driver diskette,
     you must type:

        cd /dev
        mv dsk/f0 dsk/f0.org ; mknod dsk/f0 b 2 132
        mv rdsk/f0 rdsk/f0.org ; mknod rdsk/f0 c 2 132

     NOTE: if the diskette is of 720KB (3"1/2), replace the above
     commands with:
        cd /dev
        mv dsk/f0 dsk/f0.org ; mknod dsk/f0 b 2 164
        mv rdsk/f0 rdsk/f0.org ; mknod rdsk/f0 c 2 164

A.2) For SCO 3.2v4

     To prepare the installation for 360KB (5"1/4) driver diskette,
     you must type:

        cd /dev
        mv dsk/finstall dsk/finstall.org ; mknod dsk/finstall b 2 132
        mv rdsk/finstall rdsk/finstall.org ; mknod rdsk/finstall c 2 132

     NOTE: if the diskette is of 720KB (3"1/2), replace the above
     commands with:
        cd /dev
        mv dsk/finstall dsk/finstall.org ; mknod dsk/finstall b 2 164
        mv rdsk/finstall rdsk/finstall.org ; mknod rdsk/finstall c 2 164

B) At the prompt, type

        installpkg

   >> NOTE : As some minor bug in the command "installpkg"(3.2v2), it <<
   >>        may take a while for the system to response, and DO NOT  <<
   >>        hit any key during this period.                          <<

C) Press <Enter> to install from floppy driver 0

D) Press <Enter> to install the driver

E) Press <Enter> to choose the SCO UNIX is being installed

F) Type "y" to reboot the system

G.1) Restore the original filename modified in step <A> accordingly:

     For 360KB (5"1/4) diskette, type
        cd /dev
        mv dsk/finstall.org dsk/finstall
        mv rdsk/finstall.org rdsk/finstall

     For 720KB (3"1/2) diskette, type
        cd /dev
        mv dsk/finstall.org dsk/finstall
        mv rdsk/finstall.org rdsk/finstall

<DRIVER REMOVAL>

To remove the driver,

A) At the prompt, type

        removepkg

B) Type the corresponding number of:

   "IDE32C Cache Controller Driver Package"

C) Press <Enter> to remove IDE32C driver

D) Press <Enter> to reboot
