Note for  EISA mainboards (ISA, PCI/ISA, ...)
=============================================
NetWare can not include memory above 16MB. This memory must be included
using "REGISTER MEMORY". Important is that "REGISTER MEMORY" must be
used _BEFORE_ loading the disk driver. Because "REGISTER MEMORY" can only
be used in AUTOEXEC.NCF (not in STARTUP.NCF) the disk driver also has
to be loaded there. Before loading the disk driver the volumes are not
mounted; because of this the AUTOEXEC.NCF must be on the DOS-Partition
in the same directory where SERVER.EXE is.


Note for NetWare 2.xx and NetWare3.10
=====================================
Drivers for NetWare 2.xx (only ISA and EISA) can be
downloaded from our BBS +49-7131-5972-15  in "File Area" 
"Drivers and Tools" "Netware" in the selfextracting file File NETWARE2.EXE
(please check the corresponding readme file you get with the drivers)

Further Notes
=============
- The Hot-Plug Function is in GDTMON included
  (View / Change Settings - Array Drives - Hot Plug: Replace Drive)
- To use network-functions (remote GDTMON, mail or SNMP utility)
  CTRLSRV.NLM must be loaded (see also CTRLSRV.CFG)

