HAM driver for Netware 5 or 5.1
===============================


Install NetWare 5 and 5.1
=========================

Install a NetWare 5.xx with the GDTRX.HAM driver:
- please start the installation with boot from CDROM
- press INS in the storage controller driver menue
- press F3 and change the path in A:\5.xx then press Enter
- select the GDTRX.HAM driver
- afterward complete the installation

- Recommendation: Install all patches and updates from Novell



Update an existing installation
===============================

- load NWCONFIG.NLM
- select driver options, Storage Controller Setup
- unload old drivers
- press INS to add a controller
- press F3 and change the path in A:\5.xx
- select the GDTRX.HAM driver and press Enter
- exit the install routine after the driver is loaded
- restart your Server

- Recommendation: Install all patches and updates from Novell



Install ICP Tools (icpcon and remote access tool)
=================================================

- copy all files and directories of the HAM directory to a floppy disk 
  and use this disk for the installation of NetWare
- start the installation with LOAD INSTALL.NLM
- select Product Options, Products not listed and press INS
- press F3 and edit the path to A:\5.xx and press Enter
  (if you use the driver cdrom the path is Volume:Drivers\Netware\HAM\5.xx )
- after the files are copied the tools are installed and can be started:
  LOAD ICPCON.NLM or LOAD CTRLIPX.NLM
- before you can start the CTRLIPX.NLM correctly please create a group
  ICP_Operator in the NDS and add the Admin and all other useres which 
  should be able to use this interface
- after this you can start ICPCON.EXE or ICP RAID Navigator from a 
  workstation use a user name of the group ICP_Operator and his NetWare 
  password


*** End Of File ***