fli4l documentation - Configuration

2. Basic configuration - Introduction

This chapter describes the file `config.txt` which is used for the configuration of the FLI4L router.

This file may be changed and/or edited by using a text editor or a Windows configuration software. With the help of this "fli4l wizard" you may collect all the necessary settings by just clicking with the mouse button... The whole program was redesigned and totally re-created for FLI4L version 1.4 by Carsten Cerny and Jürgen Bauer. This software´s aim is, to enable the user to generate a standard router configuration without lots of networking knowledge. Not all of the special features of FLI4L are produceable with this software version but it is a good choice for generation of a standard router configuration. Since fliwiz generates a text file (ASCII) as configuration file, the user may decide if the better solution will be fliwiz or just a text editor.

If there are any thoughts about enhancements of the program, Carsten (carsten.cerny@cc13.com) or Jürgen (jb@idowa.de) will be pleased to hear from you via email. The actual version of fliwiz can be found - as FLI4L itself - in

http://www.fli4l.de

If you want to do changes which extend the described settings and options, you will need a running Linux system to edit the rootfs. In this case you may have a look to `src/README` .

##### [ top ]