fli4l FAQ

www.fli4l.de
fli4l_FAQ's
General questions
General questions: DSL
Functions of fli4l
Problems with fli4l (only in german)
Portforwarding
...Example file

General DSL questions

Q: | I do not understand the routing settings. How do I set a correct default route to the DSL modem ?

A:

DSL makes only sense in conjunction with a default route, since this kind of connection leads to the internet. Therefore you will not find any configuration variable for this. But you may connect default routes to several circuits, which may be controlled via imonc. Thatīs useful if DSL is corrupt.

Q: | Will the network adaptor which is connected to the DSL modem automatically get a dynamical IP address ?
A: | No; the network adapter which is connected to the DSL modem wonīt get any IP address, because PPPoE will be used instead of IP.

Q: | Wille the DSL modem get an IP address, since the network adapter in the firewall owns a fixed address ?
A: | No; the DSL modem wonīt have an IP adrees either. It is only used for the physical connection. Your router will get a dynamic IP address on "DSL side". This address will only exist in a small piece of software in the router (pppd with pppoe).

Kontakt

© Copyright StPeiser