; CMD PCI-0646U PCI-0648 Bus Master Ultra DMA PCI to IDE Controller
; INF file for miniport driver
[version]
signature="$WINDOWS 95$"
Class=hdc
Provider=%CMD%

;Class Install
[ClassInstall]
AddReg=SCSI_Class

[SCSI_Class]
HKR,,,,%SCSIClassName%
HKR,,Icon,,-9

[Manufacturer]
%CMD%=CMD_HDC

[CMD_HDC]
%PCI\VEN_1095&DEV_0648.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0648
%PCI\VEN_1095&DEV_0646.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0646
%PCI\VEN_1095&DEV_0646U.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0646&REV_03
%PCI\VEN_1095&DEV_0646U2.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0646&REV_05
%PCI\VEN_1095&DEV_0646U2.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0646&REV_07
%PCI\VEN_1095&DEV_0643.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0643
%PCI\VEN_1095&DEV_0643U.DeviceDesc%=DUAL_DMA_IDE, PCI\VEN_1095&DEV_0643&REV_06
%MF\DMAPRIMARY.DeviceDesc% = P_DMA_IDE, MF\DMAPRIMARY
%MF\DMASECONDARY.DeviceDesc% = S_DMA_IDE, MF\DMASECONDARY

[P_DMA_IDE]
CopyFiles=DLLlib,@CSA64XX.MPD,@cmdide.vxd
AddReg = DmaIde_AddReg

[S_DMA_IDE]
CopyFiles=DLLlib,@CSA64XX.MPD,@cmdide.vxd
AddReg = DmaIde_AddReg

[P_DMA_IDE.HW]
AddReg=P_DmaIde_AddReg.RegHW

[S_DMA_IDE.HW]
AddReg=S_DmaIde_AddReg.RegHW

[DUAL_DMA_IDE]
AddReg=PCIMF.Reg,IDEProp.Reg
UpdateInis=Update_IOS_INI

[Update_IOS_INI]
IOS.INI,SafeList,"cmd646x.dck","cmd646x.dck",0

[DUAL_DMA_IDE.HW]
AddReg=DUAL_DMA_IDE.RegHW

[DUAL_DMA_IDE.RegHW]
HKR,Child0000,HardwareID,,MF\DMAPRIMARY
HKR,Child0000,ResourceMap,1,00,01,02,06
HKR,Child0000,MFFlags,1,0c,00,00,00
HKR,Child0001,HardwareID,,MF\DMASECONDARY
HKR,Child0001,ResourceMap,1,03,04,05,07
HKR,Child0001,MFFlags,1,0c,00,00,00
HKR,,PCIDualIDE,1,01

[DmaIde_AddReg]
HKR,,DriverDesc,,"CMD IDE Ultra DMA MiniPort Driver"
HKR,,DevLoader,,*IOS
HKR,,PortDriver,,CSA64XX.MPD
HKR,,EnumPropPages,0,"CMDIDE.DLL,EnumPropPages"

[P_DmaIde_AddReg.RegHW]
HKR,,AdapterSettings,0,%PrimaryChannelSettings%

[S_DmaIde_AddReg.RegHW]
HKR,,AdapterSettings,0,%SecondaryChannelSettings%

[PCIMF.Reg]
HKR,,DevLoader,,*CONFIGMG
HKR,,Enumerator,,*CONFIGMG
HKR,,CMDrivFlags,1,03,00,00,00

[DLLlib]
CMDide.dll

[IDEProp.Reg]
HKR,,EnumPropPages,,"sysclass.dll,IDEEnumPropPages"

[DontStopChild.RegHW]
HKR,,ConfigFlags,1,80,00,00,00

[DestinationDirs]
DLLlib = 11
DefaultDestDir = 12

[SourceDisksFiles]
csa64xx.mpd=1
cmdide.dll=1
cmdide.vxd=1

[SourceDisksNames]
1="CMD Installation Diskette",Disk1,0000-0000

[Strings]
SCSIClassName            = "Hard disk controllers"
CMD="CMD Technology"
PCI\VEN_1095&DEV_0648.DeviceDesc="CMD PCI-0648 Ultra DMA IDE Controller"
PCI\VEN_1095&DEV_0646.DeviceDesc="CMD PCI-0646 DMA IDE Controller"
PCI\VEN_1095&DEV_0646U.DeviceDesc="CMD PCI-0646U Ultra DMA IDE Controller"
PCI\VEN_1095&DEV_0646U2.DeviceDesc="CMD PCI-0646U2 Ultra DMA IDE Controller"
PCI\VEN_1095&DEV_0643.DeviceDesc="CMD PCI-0643 DMA IDE Controller"
PCI\VEN_1095&DEV_0643U.DeviceDesc="CMD PCI-0643U Ultra DMA IDE Controller"
MF\DMAPRIMARY.DeviceDesc= "Primary CMD Ultra DMA Bus Master IDE Controller"
MF\DMASECONDARY.DeviceDesc= "Secondary CMD Ultra DMA Bus Master IDE Controller"
PrimaryChannelSettings="111c10"
; PrimaryChannelSettings should be "111410" for docking stations
SecondaryChannelSettings="111c20"
; SecondaryChannelSettings should be "111420" for docking stations

