CMD PCI646X 32-Bit Local Bus IDE Driver for Netware
---------------------------------------------------

The CMD C646X3X hard disk driver can be run on Netware 3.11 and 
Netware 3.12.  It supports up to 2 IDE channels. 

Note that the CMD 32-Bit Local Bus IDE driver for DOS has to be loaded in 
CONFIG.SYS in order for the C646X3X Netware driver to function properly.

The C646X3X driver will inherit the drive mode and timing setting from DOS
driver.  There is no option to specify for this driver.  It will automatically
look for all the drives on the IDE channel(s).

To install the CMD Netware 3.x driver, run INSTALL.EXE.
