                        HighPoint Technologies, Inc.

                     HPT366 Host Adapter Device Driver 
                        
                         BIOS Revision 1.25.0

#############################################################################
Revision History:
    1.25.0  04Apl00
            . Fix problems with Diamond Fireport 40 SCSI adapters

    1.24.0  06Mar00
            . Add IC controller revision control
            . Users need to update related OS drivers if cuurent BIOS v1.24
              or above is used

    1.23.0  28Jan99
            . Increase delay time while scanning devices. Some devices need 
              more time to be ready after reset

    1.22.0  . Fix compatability problem of Seagate Barracuda hard disks
            
    1.21.0  . Fix BIOS display overlapped with SCSI type controller. BIOS
              should clean up screen whenever the initialization is done.
            . Fix BIOS not be recognized on certain PCI slot. This is
              caused by BIOS scanning the wrong PCI slot address.

    1.20.0  . Change BIOS interface to allow users to alter disk timing mode
              and select bootable disk on U66 channels.

            . Fix not compatible with Phoneix BIOS which is caused by
              the Int13h extend functions implementation in previous changes.
            . Fix compatibility with AOpen AX6BC Pro mainboard.          

    1.10.0  . Fix interrupt problem which will cause system won't
              boot up if HPT366 plugs in different PCI slots.
            . Add Int13h extended functions which are required for WHQL.

    1.00.9  . Fix compatibility problem on WD205AA hard disk.

    1.00.8  . Fix timing table setting on PIO1/PIO0 and DMA1.
            . Fix scanning error on Intel 810 chipset.
            . Fix ZIP drive problem.
            . Fix detection devices problem if only "Slave" channel.
              device exists
 
    1.00.7  . Support more than one HPT366 adapters on NT4.0 system.
    1.00.0  . Offical release.

#############################################################################


