[version]
Signature="$WINDOWS NT$"
Class=hdc
ClassGuid={4D36E96A-E325-11CE-BFC1-08002BE10318}
Provider=%CMD%
DriverVer=07/12/2000
CatalogFile=cmdide.cat


[SourceDisksNames]
1 = "CMD Installation disk",,,

[SourceDisksFiles]
cmdide.sys = 1
cmdide.inf = 1

;Class Install
[ClassInstall32.NT]
AddReg=HDC_Class

[HDC_Class]
HKR,,,,%HDCClassName%
HKR,,Icon,,"-9"
HKR,,Installer32,,"SysSetup.Dll,HdcClassInstaller"

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[Manufacturer]
%CMD%=CMD_HDC

[CMD_HDC]
%PCI\VEN_1095&DEV_0646U2.DeviceDesc%=cmdide_Inst, PCI\VEN_1095&DEV_0646&REV_05
%PCI\VEN_1095&DEV_0646U2.DeviceDesc%=cmdide_Inst, PCI\VEN_1095&DEV_0646&REV_07
%PCI\VEN_1095&DEV_0648.DeviceDesc%=cmdide_Inst, PCI\VEN_1095&DEV_0648
%PCI\VEN_1095&DEV_0649.DeviceDesc%=cmdide_Inst, PCI\VEN_1095&DEV_0649

[cmdide_Inst]
CopyFiles = @cmdide.sys

[cmdide_Inst.Services]
AddService = cmdide, %SPSVCINST_ASSOCSERVICE%, cmdide_Service_Inst

[cmdide_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\cmdide.sys
LoadOrderGroup = System Bus Extender

[cmdide_Inst.PosDup]            ;; BUGBUG: What does this do?
*PNP0600

[Strings]
HDCClassName            = "IDE ATA/ATAPI controllers"
CMD="CMD Technology"
PCI\VEN_1095&DEV_0646U2.DeviceDesc="CMD PCI-0646U2 Ultra DMA IDE Controller"
PCI\VEN_1095&DEV_0648.DeviceDesc="CMD PCI-0648 Ultra DMA IDE Controller"
PCI\VEN_1095&DEV_0649.DeviceDesc="CMD PCI-0649 Ultra DMA IDE Controller"

;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ          = 0x00020000
REG_DWORD              = 0x00010001
REG_MULTI_SZ           = 0x00010000

