HAM driver for Netware 4.10
==========================

Install a Netware 4.10
======================

Install a NetWare 4.10 with the GDTRX.HAM driver:
- please start the installation from CDROM with INSTALL.BAT
- press INS in the storage controller driver menue
- press F3 and change the path in A:\4.10 and press Enter
- SELECT FIRST CTRLTRAN.HAM and press Enter
- select the GDTRX.HAM driver and press Enter
- load other HAM drivers if necessary
- complete the installation according to the Novell instructions

- Recommendation: Install all patches and updates from Novell


Update an existing installation
===============================

- edit STARTUP.NCF
- disable the line(s) LOAD GDTRP???.DSK from the STARTUP.NCF file 
  with the character  #  at the beginning of the line(s)
  e.g.   # LOAD GDTRP400.DSK
- if other DSK drivers are installed on the system they also have 
  to be disabled and replaced by HAM drivers.
  NOTE: Before removing, please check if they are available by 
        the respective manufacturer!
- save the STARTUP.NCF file
- restart your Server
- type a Server name and a Server number in
- load INSTALL.NLM
- in Storage Controller Setup please press INS to add a controller
- press F3 and change the path in A:\4.10
- SELECT FIRST CTRLTRAN.HAM and press Enter
- select the GDTRX.HAM driver and press Enter
- load other HAM drivers if necessary
- exit the install routine after the driver is loaded
- restart your Server

- Recommendation: Install all patches and updates from Novell


Install ICP Tools (icpcon and remote access tool)
=================================================

- copy all files and directories of the HAM directory to a floppy disk and 
  use this disk for the installation of NetWare
- start the installation with LOAD INSTALL.NLM
- select Product Options, Products not listed and press INS
- press F3 and edit the path to A:\4.10 and press Enter
  (if you use the driver cdrom the path is Volume:Drivers\Netware\HAM\4.10 )
- after the files are copied the tools are installed and can be started:
  LOAD ICPCON.NLM or LOAD CTRLIPX.NLM
- before you can start the CTRLIPX.NLM correctly please create a group
  ICP_Operator with SYS:PUBLIC\SYSCON.EXE and insert the Supervisor and all
  other useres which should be able to use this interface as User
- after this you can start ICPCON.EXE or ICP RAID Navigator from a workstation
  use a user name of the group ICP_Operator and his NetWare password


*** End Of File ***